|  |  |
| --- | --- |
|  | 16-bit Five Stage MIPS Processor |
|  |  |
|  | Jared Mann V00187636, Taylor Long V00862856  CENG 450: Computer Systems and Architecture  3/30/17 |

Contents

[I. Objective 3](#_Toc478041447)

[Abstract 3](#_Toc478041448)

[Project Objective 3](#_Toc478041449)

[II. Design Requirement 3](#_Toc478041450)

[General Design Requirements 3](#_Toc478041451)

[Instruction Set 3](#_Toc478041452)

[Registers and Memory 3](#_Toc478041453)

[Pipelining 3](#_Toc478041454)

[Program Execution 3](#_Toc478041455)

[General Implementation 3](#_Toc478041456)

[III. System 4](#_Toc478041457)

[System Hierarchy Breakdown 4](#_Toc478041458)

[System Schematic Breakdown 4](#_Toc478041459)

[IV. Individual Module Design 4](#_Toc478041460)

[Top Level Processor Unit 4](#_Toc478041461)

[CPU 4](#_Toc478041462)

[ALU 4](#_Toc478041463)

[Muxes 4](#_Toc478041464)

[Program Counter 4](#_Toc478041465)

[Pipeline Registers 4](#_Toc478041466)

[RAM Module 4](#_Toc478041467)

[ROM Module 4](#_Toc478041468)

[Register File 4](#_Toc478041469)

[Control Unit 4](#_Toc478041470)

[V. Simulation Result 4](#_Toc478041471)

[VI. Analysis and Discussion 4](#_Toc478041472)

[VII. Conclusion 4](#_Toc478041473)

[VIII. Appendices 4](#_Toc478041474)

[IX. References 4](#_Toc478041475)

# Objective

## Abstract

Modern processors implement pipelining to increase throughput. Many current processors implement pipelining with various stage depths having more than 5 stages such as Intel, AMD, and even current ARM processors. Pipelining is a standard across all modern architecture designs.

## Project Objective

Build a processor; using VHDL to describe the processor, and Xilinx to synthesize and implement the design on a Spartan 3E FPGA.

# Design Requirement

## General Design Requirements

### Instruction Set

The project must implement a 16-bit RISC-like instruction set. Following the format outlined on the lab website. (Dimopolous & Hazmi, 2017) The instructions are all 1-word long.

The processor must handle three types of instructions:

* A-Format (arithmetic instructions)
* B-Format (branch instructions)
* L-Format (load and store instructions)

### Registers and Memory

Registers and Memory require certain implementations:

* 8 16-bit general purpose registers, each 1-word long, with word alignment.
* A memory address space that is byte addressable.

### Pipelining

The design must implement pipelining, using a 5 stage MIPS-like pipeline. All pipeline hazards must be handled.

### Program Execution

Regarding these types of instructions, the processor must be able to execute any program written using this instruction set. All RAW and WAR hazards must be handled.

## General Implementation Choices

# System

## System Hierarchy Breakdown

## System Schematic Breakdown

# Individual Module Design

## Top Level Processor Unit

## CPU

### ALU

### Muxes

### Program Counter

### Pipeline Registers

### RAM Module

### ROM Module

### Register File

## Control Unit

# Simulation Result

## Format A Instructions

## Format B Instructions

## Format L Instructions

# Analysis and Discussion

## Hardware Verification Procedures

# Conclusion

# Appendices

# References